**Highlights**

* Efficient producing double-sided YBCO thin films in batch with pulsed inject MOCVD
* Good homogeneity in-plane and consistency for both sides of the films
* Good consistency and repetition for this method